**ATTACHMENT A**

This Solicitation is a Contract Document and is a request for proposal in connection with the Contract awarded by the ODOC as more particularly described below. Any defined term used herein but not defined herein shall have the meaning ascribed in the General Terms or other Contract Document.

**PURPOSE**

The Contract is awarded on behalf of the Oklahoma Department of Corrections (ODOC) for commercial doors to be used at John Lilley Correctional Center in Boley, OK.

**BACKGROUND**

ODOC wishes to procure commercial doors to be delivered to John Lilley Correctional Center.

**1.** **Contract Term and Renewal Options**

This Contract is a one-time purchase.

**2.** **Scope of Work**

The parties agree to the following terms in addition to obligations set forth in other Contract Documents and provide pricing.

Commercial Doors and Accessories

* All Doors Shall Be ADA Compliant
* All Doors Shall Be UL Listed, if Applicable
* All Doors Shall Be Fully Assembled When Delivered, with Exception of Glass.
* Supplier Will Be Responsible for Installing Glass On-Site
* All Hardware Shall Be Satin Chrome In Color.

In accordance with Bidder Instructions 9.3, all manufacturers’ names, brand names,

information, and/or catalog numbers listed in a specification are for informational

purposes and not intended to limit competition and (ii) a Bidder may offer any brand for

which it is an authorized representative, which meets or exceeds the specification for any tem(s). Bidder shall offer new items of current design and technology unless the State specifies older models or versions, or used, reconditioned, or remanufactured products are acceptable. Warranties in either case should be the same. However, if a Bid is based on equivalent products, the Bid is required to state the manufacturer’s name and number. The Bid shall also explain in detail how the proposed equivalent will meet the specifications and not be considered an exception thereto.

**“The parties agree to the following terms in addition to obligations set forth in other Contract Documents and provide pricing as all-inclusive for the below.**

$\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_”

3 ea. Electric Strikes. Securitron UnLatch MUNL-24.

**Group 1**

**Exterior – Gatehouse**

2 Ea. Welded Frames

* 1-Left Hand
* 1-Right Hand
* 3070-7"X4” Header-16 Gauge-Closer
* Reinforced Existing Wall Anchors

2 Ea. Doors- Closed Top

* 1-Right Hand Reverse
* 1-Left Hand Reverse
* 3070-1 3/4” 18 Gauge-Government 86 Cut Out
* Lite Kits Lopro-24"x24"-LK

2 Ea. Lite Kit Low Profile 24”X24” LK

6 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

2 Ea. Double Cylinder Mortise Deadlock. Corbin Russwin ML2022-LWN-626-L/C.

4 Ea. Interchangeable Core Housings. KS407-US26DxKS702 CAM

4 Ea. Interchangeable Cores & Keys. KS207-K-US26D

2 Ea. Door Closers. LCN 4040XP-EDA-ALUM

2 Ea. Outswing Thresholds W/ Vinyl Lip 181-AV-36"

2 Ea. Sets Weatherstrip. Pemko 306-AV-36X84

**Interior – Gatehouse**

5 Ea. Welded Frames

* 3-Left Hand
* 2-Right Hand
* 3070-7”x4” Header 16 Gauge-Closer
* Reinforced Existing Wall Anchors

1 Ea. Door

* Right Hand Reverse
* 3070-1 3/4”-18 Gauge-Government 86 Cut Out
* 6” X 27” Lite Cutout

2 Ea. Doors

* Right Hand Reverse
* 3070-1 3/4”-18 Gauge-Government 86 Cut Out

2 Ea. Doors

* Left Hand Reverse
* 3070-1 3/4”-18 Gauge-Government 86 Cut Out

1 Ea. Lite Kit Lopro 6"x27"-LK

15 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Double Cylinder Mortise Deadlock. Corbin Russwin ML2022-LWN-626-L/C

3 Ea. Storeroom Mortise Locks Corbin Russwin ML2057-LWN-626-L/C

1 Ea. Double Cylinder Mortise Deadlock. Corbin Russwin ML2062-LWN-626-L/C

1 Ea. Mortise Deadbolt (Extra). Schlage L462L-626-L/C

7 Ea. Interchangeable Core Housings. KS405-US26DxKS702 Cam

2 Ea. Interchangeable Core Housings. KS405-US26DxKS702L Cam

9 Ea. Interchangeable Cores & Keys. KS207-K-US26D

5 Ea. Door Closers. LCN 4040XP-EDA-ALUM

**Welded Windows - Gatehouse**

2 Ea. 48"x48"x7" OD - EWA

10 Ea. 48"x52"X 7" OD - EWA

**Glass - Gatehouse**

2 Ea. 1/4"x23"x23" Tempered (Doors)

1 Ea. 1/4"x5"x26" Tempered (Doors)

10 Ea. 1”x44”x48” O/A Clear/Clear to fit above frames.

* SB60 Low E, Tempered, Insulated Glass Units

**Group 2**

**Door #1 - Kitchen: Front Exit Door**

1 Ea. Door

* 3070-1 3/4"-18 Gauge
* Right Hand Reverse
* Hinge Prep To Match Existing
	+ - Top Hinge 9-1/4”
		- Middle Hinge 39-1/4”
		- Bottom Hinge 69-1/4”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #2 - Unit 1: A-Dorm West Door**

1 Ea. Door

* 3068-1 3/4"- 18 Gauge
* Left Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-5/8”
	+ Middle Hinge 37-5/8”
	+ Bottom Hinge 68-5/8”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

2 Ea. Door Closers. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

**Door #3 - Unit 1: SHU Door to Cages (East Side)**

1 Ea. Door

* 3068-1 3/4"-18 Gauge
* Right Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 7-3/8”
	+ Middle Hinge 37-3/8”
	+ Bottom Hinge 67-1/4”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage E L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

2 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #4 - Unit 1: C-Dorm West Door**

1 Ea. Door

* 3068-1 3/4"-18 Gauge
* Left Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-5/8”
	+ Middle Hinge 37-5/8”
	+ Bottom Hinge 68-5/8”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. SCHLAGE L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #5 - Unit 1: D-Dorm East Door**

1 Ea. Door

* 3068-1 3/4"-18 Gauge
* Left Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-5/8”
	+ Middle Hinge 37-3/4”
	+ Bottom Hinge 68-3/4”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. SCHLAGE L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #6 - Unit 1: E-Dorm West Door**

1 Ea. Door

* 3068-1 3/4"-18 Gauge
* Left Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-5/8”
	+ Middle Hinge 37-5/8”
	+ Bottom Hinge 68-5/8”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #7 - Unit 1: F-Dorm East Door**

1 Ea. Door

* 3068-1 3/4"-18 Gauge
* Right Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-3/4”
	+ Middle Hinge 37-3/4”
	+ Bottom Hinge 68-3/4”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For SCHLAGE L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* 1 Right Hand
* 1 Left Hand

**Door #8 - Unit 2: G-Dorm East**

1 Ea. Door

* 3070-1 3/4"-18 Gauge
* Right Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 4-7/8”
	+ Middle Hinge 37-1/8”
	+ Bottom Hinge 69-3/8”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. SCHLAGE L462L-626-L/C

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

2 Ea. Plates. Rockwood 91-CFC-US32D

* + - 1 Right Hand
		- 1 Left Hand

**Door #9 - Warehouse: Old Maintenance Entrance**

1 Ea. Welded Frame

* 3070-5 3/4"-16 Gauge
* Left Hand
* Hinge Prep To Match Existing
* Existing Wall Anchors

1 Ea. Door

* 3070-1 3/4"-18 Gauge Government 86 Cut Out
* Right Hand Reverse
* Hinge Prep To Match Existing
* Closed Top. Heavy Duty Hinge Prep Closer

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C-RHR

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

**Door #10 - Administration: Leisure Library**

1 Ea. Welded Frame

* + 3070-5 3/4"-16 Gauge
	+ Right Hand
	+ Hinge Prep To Match Existing
	+ Existing Wall Anchors

1 Ea. Door

* 3070-1 3/4"-18 Gauge Government 86 Cut Out
* Right Hand Reverse
* Hinge Prep To Match Existing
* Closed Top. Heavy Duty Hinge Prep Closer

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C-LHR

2 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

2 Ea. Interchangeable Cores & Keys. KS207-K-US26D

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

**Door #11 - Administration: South Door Atop Stairs**

1 Ea. Welded Frame

* + 3070-5 3/4"-16 Gauge
	+ Left Hand
	+ Hinge Prep To Match Existing
	+ Existing Wall Anchors

1 Ea. Door

* 3070-1 3/4"-18 Gauge Government 86 Cut Out
* Right Hand Reverse
* Hinge Prep To Match Existing
* Closed Top. Heavy Duty Hinge Prep Closer

3 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

1 Ea. Mortise Deadlock. Schlage L462L-626-L/C-RHR

1 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

1 Ea. Door Closer. LCN 4040XP-EDA-ALUM

**Door #12 - Gymnasium: 2 Front Doors**

2 Ea. Door

* 3070-1 3/4"-18 Gauge
* Left Hand Reverse
* Hinge Prep To Match Existing
	+ Top Hinge 6-1/2”
	+ Middle Hinge 39-1/2”
	+ Bottom Hinge 72-1/2”
* Closed Top. Heavy Duty Hinge Prep, Closer
* Reinforced Prep For Schlage L462 Double Cylinder

6 Ea. Heavy Duty Hinges. PBB 4B81-4.5”x4.5”-US26D-NRP

2 Ea. Mortise Deadlock. Schlage L462L-626-L/C

4 Ea. Interchangeable Core Housings. KS407-US26D-KS702 Cam

4 Ea. Interchangeable Cores & Keys. KS207-K-US26D

2 Ea. Door Closer. LCN 4040XP-EDA-ALUM

4 Ea. Plates. Rockwood 91-CFC-US32D

* 2 Right Hand
* 2 Left Hand